For 1990-2009 cars

### Removal Procedure

1. Insert a small, flat-bladed tool between repeater lamp and vehicle front fender.
2. Use the small, flat-bladed tool to compress the repeater lamp retaining tab.
3. Remove the repeater lamp from the front fender.
4. Disconnect the electrical connector.
5. Remove the repeater lamp from the vehicle.

### Installation Procedure

1. Connect the electrical connector to the repeater lamp.
2. Align the repeater lamp retaining tabs with the slots in the front fender.
3. Push the repeater lamp into the hole in the front fender until the retaining tabs snap into place