For 1990-2009 cars

### Removal Procedure

1. Relieve fuel system pressure. Refer to Fuel Pressure Relief .
2. Drain fuel tank. Refer to Fuel Tank Draining .
3. Remove the fuel tank. Refer to Fuel Tank Replacement .
4. Remove the fuel sender assembly. Refer to Fuel Sender Assembly Replacement .
5. Remove the fuel level sensor (5) from the modular fuel sender.

### Installation Procedure

1. Install the fuel level sensor (5) to the modular fuel sender.
2. Install the fuel sender assembly. Refer to Fuel Sender Assembly Replacement .
3. Install the fuel tank. Refer to Fuel Tank Replacement .
4. Lower the vehicle.
5. Add fuel and Install the fuel fill cap.
6. Inspect for fuel leaks using the following procedure:

6.1. | Turn ON the ignition, for 2 seconds.

6.2. | Turn OFF the ignition, for 10 seconds.

6.3. | Turn ON the ignition.

6.4. | Inspect for fuel leaks.