For 1990-2009 cars

### Removal Procedure

Important: Remove the luggage carrier as an assembly.

1. Remove the front and rear mounting screws from the luggage carrier.
2. Remove the center mounting screws, if equipped, from the luggage carrier.
3. Remove the luggage carrier from the roof with an assistant.

### Installation Procedure

1. Position the luggage carrier to the roof with an assistant.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the center mounting screws, if equipped, to the luggage carrier.

Tighten
Tighten the screws to 6 N·m (53 lb in).

3. Install the front and rear mounting screws to the luggage carrier.

Tighten
Tighten the screws to 6 N·m (53 lb in).