For 1990-2009 cars

### Removal Procedure

1. Remove the sliding door inner trim panel. Refer to Sliding Door Inner Trim Panel Replacement .
2. Remove the sliding door water deflector. Refer to Rear Side Door Water Deflector Replacement .
3. Disconnect the power sliding door latch release actuator electrical connector.
4. Remove the power sliding door latch release actuator screws.
5. Remove the power sliding door latch release actuator.
6. Unhook the power sliding door latch release actuator rod from the power sliding door latch release actuator.

### Installation Procedure

1. Install the power sliding door latch release actuator rod to the power sliding door latch release actuator.
2. Install the power sliding door latch release actuator to the power sliding door.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the power sliding door latch release actuator screws.

Tighten
Tighten the screws to 10 N·m (89 lb in).

4. Install the sliding door water deflector. Refer to Rear Side Door Water Deflector Replacement .
5. Install the sliding door inner trim panel. Refer to Sliding Door Inner Trim Panel Replacement .