For 1990-2009 cars

### Removal Procedure

1. Use a small, flat-bladed tool in order to remove the cargo lamp from the headliner.
2. Disconnect the electrical connectors from the cargo lamp.
3. Remove the cargo lamp from the headliner.
4. Use a small, flat-bladed tool in order to remove the cargo lamp lens from the cargo lamp.
5. Use a small, flat-bladed tool in order to remove the bulb from the socket.

### Installation Procedure

1. Press the bulb into the socket.
2. Snap the cargo lamp lens into the cargo lamp.
3. Connect the electrical connectors to the cargo lamp.
4. Install the cargo lamp to the headliner.
5. Snap the cargo lamp into place.