For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

### Removal Procedure

1. Remove the bolts from the fender splash shield.
2. Use J 38778 in order to remove the push-in retainer from the lower fender splash shield at the rocker panel.
3. Remove the fender splash shield from the fender.

### Installation Procedure

1. Align the locating pins on the fender splash shield into the holes in the fender.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts to the fender splash shield.

Tighten
Tighten the bolts to 2 N·m (18 lb in).

3. Install the push-in retainer to the lower fender splash shield at the rocker panel.