For 1990-2009 cars

Condition | Action
--- | ---
The fluid level is low. |

1. Inspect for a fluid leak.

Refer to Power Steering Gear and Pump Leaks .

2. Add fluid as needed.

Refer to Checking and Adding Power Steering Fluid .

The pressure plates are scored. | Replace the components as needed. Refer to Power Steering Pump Replacement .
The vanes are scored. | Replace the components as needed. Refer to Power Steering Pump Replacement .
The pump bushing is scored. | Replace the pump brush as needed. Refer to Power Steering Pump Replacement .