For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad Clip Remover

### Removal Procedure

1. Remove the rear seats. Refer to Rear Seat Replacement in Seats.
2. Remove the back body pillar trim. Refer to Upper Rear Trim Finish Panel Replacement .
3. Remove the body side upper trim panel. Refer to Third Pillar Trim Replacement .
4. Remove the cup holder from the rear quarter trim.
5. Remove the rear accessory panel, for the left side quarter panel. Refer to Rear Accessory Panel Replacement .
6. Remove the seat belt retractor retainer bolt. Refer to Rear Seat Belt Retractor Replacement in Seat Belts.
7. Remove the upper cargo net retainers.
8. Remove the liftgate sill plate. Refer to Liftgate Door Sill Plate Replacement .
9. Remove the rear quarter trim panel retainers using J 38778 .
10. Remove the rear quarter trim panel from the vehicle.

### Installation Procedure

1. Install rear quarter trim panel to vehicle.
2. Install the rear quarter trim retainers by aligning the retainer with the holes and then pushing the retainers to secure.
3. Install the upper cargo net retainers.
4. Install the liftgate sill plate. Refer to Liftgate Door Sill Plate Replacement .
5. Install the seat belt retractor retaining bolt. Refer to Rear Seat Belt Retractor Replacement in Seat Belts.
6. Install the rear accessory panel, for the left side quarter panel. Refer to Rear Accessory Panel Replacement .
7. Install the cup holder to the rear quarter trim.
8. Install the body side upper trim panel. Refer to Third Pillar Trim Replacement .
9. Install the back body pillar trim. Refer to Upper Rear Trim Finish Panel Replacement .
10. Install the rear seats. Refer to Rear Seat Replacement in Seats.