For 1990-2009 cars

1. Disconnect the cruise control cable at the module and the throttle lever. Refer to Cruise Control Cable Replacement .
2. Ensure that the cruise control cable moves in and out of the cable casing in the following manner:

• | Freely

• | Smoothly

3. Replace any sticking or binding cables. Refer to Cruise Control Cable Replacement .
4. Replace any cable that contains an adjuster lock that does not hold under normal operating conditions. Refer to Cruise Control Cable Replacement .