For 1990-2009 cars

1. Install a new 3-4 accumulator piston cylinder O-ring seal (422) onto the 3-4 accumulator piston cylinder (421).
2. Install the 3-4 accumulator piston outer spring (423) and inner spring (424) into the 3-4 accumulator piston cylinder (421).
3. Install a new 3-4 accumulator piston seal (427) onto the 3-4 accumulator piston (428).
4. Insert the 3-4 accumulator piston (428) into the 3-4 accumulator piston cylinder (421).
5. Using a slight twisting motion, insert the 3-4 accumulator piston cylinder (421) into the case cover (401).
6. Insert the 3-4 accumulator piston pin (426) through the front of the case cover (401) and into the 3-4 accumulator piston (428).
7. Install the manual valve (404) into the case cover (401).
8. Install the actuator feed limit valve (414) into the case cover (401).
9. Install the actuator feed limit valve spring (415) into the case cover (401).
10. Install the actuator feed limit valve spring retainer (416) into the case cover (401).