For 1990-2009 cars

#### Tools Required

• | J 8092 Driver Handle

• | J 41991 Driveshaft Bearing Remover/Installer

1. Assemble J 8092 and J 41991 for bearing installation.
2. Place the case cover (400) on a clean, flat surface with the case mating surface up.

Important: When installing the new bearing the part number should be visible (facing upward).

3. Using the assembled tool, press the drive shaft bearing (431) into the case cover (400).