For 1990-2009 cars

### Removal Procedure

1. Remove the transaxle. Refer to Transmission Replacement in Automatic Transaxle - 4T65-E.
2. Remove the engine flywheel. Refer to Engine Flywheel Removal .
3. Remove the crankshaft rear oil seal. Refer to Crankshaft Rear Oil Seal Removal .

### Installation Procedure

1. Install the rear main seal. Refer to Crankshaft Rear Oil Seal Installation .
2. Install the engine flywheel. Refer to Engine Flywheel Installation .
3. Install the transaxle. Refer to Transmission Replacement in Automatic Transaxle - 4T65-E.