For 1990-2009 cars

### Removal Procedure

1. Remove the wiper motor from the vehicle. Refer to Windshield Wiper Motor Replacement .
2. Remove three screws and the wiper motor cover from the wiper motor.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the wiper motor cover onto the wiper motor with three screws.

Tighten
Tighten three screws to 2 N·m (18 lb in).

2. Install the wiper motor onto the vehicle. Refer to Windshield Wiper Motor Replacement .
3. Operate the wipers and check for proper operation.