For 1990-2009 cars

### Removal Procedure

1. Carefully release the locking tabs using a flat-bladed tool in the locations as indicated.
2. Remove the second seat audio control from the overhead entertainment console.
3. Disconnect the electrical connector from the second seat audio control.

### Installation Procedure

1. Connect the electrical connector to the second seat audio control.
2. Install the second seat audio control to the overhead entertainment console.
3. Press the second seat audio control until it locks into place.