For 1990-2009 cars

## Aluminum Wheel Hub Cap Replacement Chevrolet and Oldsmobile

### Removal Procedure

1. Use a flat-bladed tool in order to pry the edge of the hub cap out.
2. Use your fingers in order to pull the hub cap off of the wheel.
3. Place the hub cap down with the finished surface facing up. Do Not place anything on top of the wheel cover.

### Installation Procedure

1. Install the hub cap to the wheel.
2. Use one hand in order to hold one side of the hub cap in.
3. Use your other hand or a rubber mallet in order to tap the outer edge of the hub cap into the wheel.

## Aluminum Wheel Hub Cap Replacement Pontiac

### Removal Procedure

1. Place a block of wood or the handle of a flat-bladed tool though the back of the wheel toward the hub cap.
2. Strike the block of wood (or flat-bladed tool end) with a hammer in order to remove the hub cap from the wheel.
3. Place the hub cap down with the finished surface facing up. Do not place anything on top of the wheel center hub cap to avoid damaging the surface.

### Installation Procedure

1. Place the wheel center hub cap into the wheel.
2. Cover the wheel center hub cap with a piece of thick cloth.
3. Use your other hand or a rubber mallet in order to install the hub cap to the wheel.