For 1990-2009 cars

### Removal Procedure

1. Relieve the system fuel pressure. Refer to Fuel Pressure Relief .
2. Drain fuel tank. Refer to Fuel Tank Draining .
3. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in Cautions and Notices.
4. Remove the fuel tank. Refer to Fuel Tank Replacement .
5. Disconnect the electrical connector from the fuel tank vapor pressure sensor.
6. Remove the fuel tank pressure sensor (7) from the modular fuel sender.

### Installation Procedure

1. Install the new fuel tank pressure sensor (7) to the modular fuel sender.
2. Connect the FTP sensor electrical connector.
3. Install the fuel tank. Refer to Fuel Tank Replacement .
4. Lower the vehicle.
5. Add fuel and Install the fuel fill cap.
6. Reconnect the negative battery cable.
7. Inspect for fuel leaks using the following procedure:

7.1. | Turn ON the ignition, for 2 seconds.

7.2. | Turn OFF the ignition, for 10 seconds.

7.3. | Turn ON the ignition.

7.4. | Inspect for fuel leaks.