For 1990-2009 cars

## Front Wheel Drive Shaft Seal Replacement Left

#### Tools Required

• | J 23129 Axle Boot Remover

• | J 6125-1B Slide Hammer

• | J 34115 Left Side Axle Seal Installer

• | J 37292-B Axle Seal Protector

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the left front tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Remove the left engine splash shield. Refer to Engine Splash Shield Replacement in Body Front End.
4. Remove the left stabilizer shaft link from the left lower control arm. Refer to Stabilizer Shaft Link Replacement in Front Suspension.
5. Remove the left tie rod end from the left steering knuckle. Refer to Rack and Pinion Outer Tie Rod End Replacement in Power Steering System.
6. Remove the left lower ball joint from the left steering knuckle. Refer to Lower Control Arm Ball Joint Replacement in Front Suspension.
7. Disconnect the left drive axle from the transaxle. Refer to Wheel Drive Shaft Replacement in Wheel Drive Shafts.
8. Secure the left drive axle to the left steering knuckle and strut.
9. Use J 23129 and J 6125-1B in order to remove the axle oil seal (409) from the case cover (401).

### Installation Procedure

1. Use a light wipe of transaxle fluid to lubricate the seal lip.
2. Use the J 34115 to install a new seal.
3. Install the J 37292-B in the seal.

Important: Carefully guide the axle shaft past the lip seal. Do NOT allow the shaft splines to contact any portion of the seal lip surface or damage to the seal will occur.

4. Connect the left drive axle to the transaxle. Refer to Wheel Drive Shaft Replacement in Wheel Drive Shafts.
5. Remove the J 37292-B .
6. Install the left lower ball joint to the left steering knuckle. Refer to Lower Control Arm Ball Joint Replacement in Front Suspension.
7. Install the left tie rod end to the left steering knuckle. Refer to Rack and Pinion Outer Tie Rod End Replacement in Power Steering System.
8. Install the left stabilizer shaft link to the left lower control arm. Refer to Stabilizer Shaft Link Replacement in Front Suspension.
9. Install the left engine splash shield. Refer to Engine Splash Shield Replacement in Body Front End.
10. Install the left front tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
11. Lower the vehicle.
12. Adjust the fluid level. Refer to the following information:

• | Transmission Fluid Check

• | Fluid and Lubricant Recommendations in Maintenance and Lubrication

• | Approximate Fluid Capacities in Maintenance and Lubrication

13. Inspect for fluid leaks.

## Front Wheel Drive Shaft Seal Replacement Right

#### Tools Required

• | J 23129 Axle Boot Remover

• | J 6125-1B Slide Hammer

• | J 29130 Right Side Axle Seal Installer

• | J 37292-B Axle Seal Protector

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the right front tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Remove the right engine splash shield. Refer to Engine Splash Shield Replacement in Body Front End.
4. Remove the right stabilizer shaft link from the right lower control arm. Refer to Stabilizer Shaft Replacement in Front Suspension.
5. Remove the right tie rod end from the right steering knuckle. Refer to Rack and Pinion Outer Tie Rod End Replacement in Power Steering System.
6. Remove the right lower ball joint from the right steering knuckle. Refer to Lower Control Arm Ball Joint Replacement in Front Suspension.
7. Disconnect the right drive axle from the transaxle. Refer to Wheel Drive Shaft Replacement in Wheel Drive Shafts.
8. Secure the right drive axle to the right steering knuckle and strut.
9. Use J 23129 and J 6125-1B in order to remove the axle oil seal (4) from the case extension assembly.

### Installation Procedure

1. Use a light wipe of transaxle fluid to lubricate the seal lip.
2. Use the J 29130 to install a new seal.
3. Install the J 37292-B in the seal.

Important: Carefully guide the axle shaft past the lip seal. Do NOT allow the shaft splines to contact any portion of the seal lip surface or damage to the seal will occur.

4. Connect the right drive axle to the transaxle. Refer to Wheel Drive Shaft Replacement in Wheel Drive Shafts.
5. Remove the J 37292-B .
6. Install the right lower ball joint to the right steering knuckle. Refer to Lower Control Arm Ball Joint Replacement in Front Suspension.
7. Install the right tie rod end to the right steering knuckle. Refer to Rack and Pinion Outer Tie Rod End Replacement in Power Steering System.
8. Install the right stabilizer shaft link to the right steering knuckle. Refer to Stabilizer Shaft Link Replacement in Front Suspension.
9. Install the right engine splash shield. Refer to Engine Splash Shield Replacement in Body Front End.
10. Install the right front tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels
11. Lower the vehicle.
12. Adjust the fluid level. Refer to the following information:

• | Transmission Fluid Check

• | Fluid and Lubricant Recommendations in Maintenance and Lubrication

• | Approximate Fluid Capacities in Maintenance and Lubrication

13. Inspect for fluid leaks.