For 1990-2009 cars

Important: The rear defogger bus bar lead wire, the antenna, or the defogger terminal can be reattached by resoldering using a solder containing 3 percent silver and a rosin flux paste.

1. Clean the repair area by buffing with fine steel wool. This removes the oxide coating formed during the window manufacture.
2. Install the paste-type rosin flux in small quantities to the rear defogger bus bar lead wire antenna or the defogger terminal repair area using a brush.

Notice: Use only enough heat to melt the solder. Using excessive heat can damage the rear window defogger components or the rear window.

3. Coat the solder iron tip with the solder.

• | Use only enough heat to melt the solder.

• | Use only enough solder to ensure a complete repair.

4. Install the solder to the feed bus bar or the ground bus bar.
5. Draw the soldering iron tip across the fluxed area, thinly coating the bus bar with solder.
6. Install a small amount of flux to the underside of the rear defogger bus bar lead wire antenna or the defogger terminal.
7. Align the spots with flux to the underside of the rear defogger bus bar lead wire, antenna, or defogger terminal.
8. Coat the tip of the soldering iron with solder.
9. Install the solder to the underside of the rear defogger bus bar lead wire antenna to the defogger terminal.
10. Draw the iron across the fluxed spot, thinly coating the spot of solder.
11. Solder the spot on the braid against the spot on the feed bus bar or the ground bus bar.

• | Use pliers in order to hold the rear defogger bus bar lead wire antenna or the defogger terminal.

• | Apply the heat to the top of the rear defogger bus bar lead wire antenna or the defogger terminal. This causes the solder spot to melt and fuse together.

• | Do not remove the holding force until the solder has solidified.

• | Wipe off the excess flux with solvent.

12. Install the electrical connector.