For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Battery | Engine compartment, behind the right headlamp | -- | --
Crank Relay | Right side of Engine Compartment on the radiator support, inboard of the underhood accessory wiring junction block | Power and Grounding Component Views | Power and Grounding Connector End Views
Data Link Connector (DLC) | Below the steering column, bottom of the knee bolster | Data Link Communications Component Views | Data Link Communications Connector End Views
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | Electrical Center Identification Views
Fusible Link A | Bolted to the starter solenoid | -- | --
Fusible Link C | Bolted to the starter solenoid | -- | --
Fusible Link K | Bolted to the starter solenoid | -- | --
Fusible Link Z | Bolted to the starter solenoid | -- | --
Generator | Top rear right side of the engine | Engine Electrical Component Views | Engine Electrical Connector End Views
Instrument Cluster | Left side of the IP | Instrument Panel, Gages, and Console Component Views | Instrument Panel, Gages, and Console Connector End Views
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views | Engine Controls Connector End Views
Splice Pack SP205 | Below the steering column, bottom of the knee bolster | Data Link Communications Component Views | Data Link Communications Connector End Views
Starter Motor | Lower front of the engine | -- | --
Starter Solenoid | Lower front of the engine, part of the starter motor assembly | -- | --
Transaxle Range Switch | Rear left side of the engine compartment, mounted to the top of the transaxle | Engine Controls Component Views | Automatic Transmission Related Connector End Views
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
C101 (20 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, near the EBCM | Harness Routing Views | Inline Harness Connector End Views
G100 | Battery grounded to the right inner fender, near the battery | Harness Routing Views | --
G113 | Engine compartment, left of the starter, along with the battery ground | Harness Routing Views | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views | --
S108 | Engine harness, front left side of the engine compartment approximately 8 cm (3 in) from the PCM breakout | -- | --
S209 | IP harness, center of the IP approximately 8 cm (3 in) from the security indicator lamp breakout | -- | --