For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad and garnish Clip Remover

### Removal Procedure

1. Open the powersliding door.
2. Using the J 38778 , remove the sliding door jamb contact plate push-in retainers.
3. Remove the sliding door jamb contact plate from the pillar.
4. Disconnect the sliding door jamb contact plate electrical connector.

### Installation Procedure

1. Connect the sliding door jamb contact plate electrical connector.
2. Position the sliding door jamb contact plate to the pillar.
3. Install the sliding door jamb contact plate push-in retainers.
4. Close the sliding door.