For 1990-2009 cars

### Removal Procedure

1. Fold down the child restraint to the open position.
2. Grasp the child restraint pad and pull in order to disengage the hook and the loop retainers.
3. Remove the child restraint pad.

### Installation Procedure

1. Install the child restraint pad.
2. Push firmly on the child restraint pad in order to secure the hook and the loop retainers.
3. Fold up the child restraint to the closed position.