For 1990-2009 cars

### Tools Required:

• | J 23327 Clutch Spring Compressor

• | J 38734 Spring Compressor Adapter

1. Use a flat blade screwdriver in order to remove the retaining ring (627) from the second clutch housing.
2. Remove the second clutch backing plate (626). Remove the alternating second clutch fiber plates (624). Remove the second clutch steel plates (625).
3. Remove the second clutch apply plate (716). Remove the second clutch waved plate (623).
4. Use J 23327 (1) and J 38734 (2) in order to compress the second clutch piston spring (621).
5. Remove the retaining ring (622).
6. Remove J 23327 and J 38734 from the second clutch housing (617).
7. Remove the second clutch spring assembly (621).
8. Remove the second clutch piston assembly (620).