For 1990-2009 cars

### Removal Procedure

Notice: Do not pry against the splash shield or backing plate in attempt to free the drum. This will bend the splash shield or backing plate. A bent backing plate may cause brake chatter and/or pulsation.

1. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
2. Remove the brake drum. Refer to Brake Drum Replacement .
3. Remove the brake shoes. Refer to Brake Shoe Replacement .
4. Remove the park brake actuator from the park brake cable.
5. Remove the park brake cable ONLY from the backing plate.

• | For the left side park brake cable replacement, refer to Parking Brake Rear Cable Replacement - Left Side .

• | For the right side park brake cable replacement, refer to Parking Brake Rear Cable Replacement - Right Side .

6. Remove the wheel cylinder (3). Refer to Wheel Cylinder Replacement .
7. Remove the wheel bearing/hub. Refer to Rear Wheel Bearing and Hub Replacement in Rear Suspension.
8. Remove the backing plate.

### Installation Procedure

1. Install the backing plate.
2. Install the wheel bearing/hub. Refer to Rear Wheel Bearing and Hub Replacement in Rear Suspension.
3. Install the wheel cylinder (3). Refer to Wheel Cylinder Replacement .
4. Install the park brake cable to the backing plate.

• | For the left side park brake cable replacement, refer to Parking Brake Rear Cable Replacement - Left Side in Park Brake.

• | For the right side park brake cable replacement, refer to Parking Brake Rear Cable Replacement - Right Side in Park Brake.

5. Install the park brake actuator to the park brake cable.
6. Install the brake shoes. Refer to Brake Shoe Replacement .
7. Install the brake drum. Refer to Brake Drum Replacement .
8. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.