For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

### Removal Procedure

1. Remove the garnish molding. Refer to Rear Side Door Garnish Molding Replacement .
2. Remove the inside handle. Refer to Sliding Door Inside Handle Replacement .
3. Use J 38778 in order to remove the inner trim panel from the sliding door.

### Installation Procedure

1. Install the inner trim panel to the sliding door.
2. Align the locating pins on the inner trim panel.
3. Firmly press on the inner trim panel in order to seat the retainers.
4. Install the inside handle. Refer to Sliding Door Inside Handle Replacement .
5. Install the garnish molding. Refer to Rear Side Door Garnish Molding Replacement .