For 1990-2009 cars

## Door Trim Panel Replacement Front Door

#### Tool Required

J 38778 Door Trim Pad Remover

### Removal Procedure

1. Open the door.
2. Remove the front door trim plate. Refer to Door Trim Plate Replacement .
3. Remove the front door manual window regulator handle if equipped. Refer to Door Window Regulator Handle Replacement .
4. Remove the armrest screws.
5. Route the electrical harness through the front door trim panel opening.
6. Use J 38778 in order to remove the front door trim panel from the door.
7. Use J 38778 in order to pry the front door trim panel from the door frame at the window seal.
8. Remove the front door trim panel from the door.

### Installation Procedure

1. Install the front door trim panel to the front door.
2. Place the window seal portion of the panel over the door frame.
3. Route the electrical harness through the front door trim panel opening and into place.
4. Align the front door trim panel retainers to the holes in the door metal.
5. Firmly press the front door trim panel to the door metal in order to seat the retainers.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

6. Install the armrest screws.

Tighten
Tighten the screws to 3 N·m (26 lb in).

7. Install the front door manual window regulator handle if equipped. Refer to Door Window Regulator Handle Replacement
8. Install the door trim plate. Refer to Door Trim Plate Replacement .
9. Close the door.