For 1990-2009 cars

1. Using a small screwdriver, pry the wiring harness (224/225) electrical connectors off of the following components:

• | Automatic transaxle fluid pressure manual valve position switch assembly (395)

• | 1-2, 3-4 Shift solenoid valve assembly (315A)

• | 2-3 Shift solenoid valve assembly (315B)

• | TCC PWM solenoid valve assembly (334)

• | Pressure control solenoid valve assembly (322)

• | Automatic transaxle input speed sensor assembly (440)

• | IMS (811)

2. Gently pull the automatic transaxle fluid temperature sensor (391) from it's clip.
3. Lift the wiring harness assembly (224/225) off of the transaxle.