For 1990-2009 cars

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the ignition and key alarm switch assembly (3) onto the electronic lock module assembly (2) and secure by using the 2 tapping screws.

Tighten
Tighten the screws to 4.7 N·m (42 lb in).

2. Install the key alarm connector (1) into the electronic lock module assembly (2).
3. Slide the PASSKEY® III (2) onto the electronic lock module assembly (1).
4. Slide the turn signal switch assembly connectors (2) to the bulkhead connector (1).

Caution: Improper routing of the wire harness assembly may damage the inflatable restraint steering wheel module coil. This may result in a malfunction of the coil, which may cause personal injury.

5. Install the wire harness assembly (4) into the wire harness strap (5).
6. Install the wire harness strap (2) into the steering column tilt head assembly (1).
7. Install the wire harness straps (3) onto the wire harness assembly (4).
8. Install the upper and lower trim covers. Refer to Steering Column Trim Covers - Assemble - Off Vehicle .
9. Enable the inflatable restraint steering wheel module. Refer to Enabling the SIR System in SIR.