For 1990-2009 cars

### Removal Procedure

1. Remove the automatic level control air compressor from the vehicle. Refer to Air Compressor Replacement .
2. Clean the area around the connection of the air dryer (2) to the automatic level control air compressor head (1).
3. Rotate the spring clip retaining the dryer to the automatic level control air compressor 90 degrees.
4. Remove the air dryer (2) from the air dryer bracket and the automatic level control air compressor.

### Installation Procedure

1. Install the air dryer (2) to the air dryer bracket (3) and automatic level control air compressor.
2. Rotate the clip 90 degrees in order to retain the dryer to the automatic level control air compressor.
3. Install the automatic level control air compressor to the vehicle. Refer to Air Compressor Replacement