For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | Electrical Center Identification Views
Heated Seat Module | Under the seat frame at rear of cushion | Power Seat Component Views | Power Seat Connector End Views
Heated Seat Switch | Part of the rear window wiper/washer and multi-function switch | Power Seat Component Views | Power Seat Connector End Views
Passenger Seat Adjuster Motor Assembly | Under the right front seat | Power Seat Component Views | Power Seat Connector End Views
Passenger Seat Adjuster Switch | Mounted to the side of the base of the right front seat | Power Seat Component Views | Power Seat Connector End Views
Rear Window Wiper/Washer and Multi-function Switch (Heated Seat Switch) | Part of the rear window wiper/washer and multi-function switch | Wiper/Washer Component Views | --
Seat Adjuster Motor Assembly | Under the front seat | Power Seat Component Views | Power Seat Connector End Views
Seat Adjuster Switch | Mounted to the side of the base of the seat | Power Seat Component Views | Power Seat Connector End Views
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | Harness Routing Views | Inline Harness Connector End Views
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views | Inline Harness Connector End Views
C313 (2 cavities) | Body wiring harness to the driver seat adjuster switch wiring harness, under the driver seat | Harness Routing Views | Inline Harness Connector End Views
C314 (2 cavities) | Body wiring harness to the passenger seat adjuster switch wiring harness, under the passenger seat | Harness Routing Views | Inline Harness Connector End Views
C315 (4 cavities) | Body wiring harness to the driver seat heater module wiring harness, under the driver seat | Harness Routing Views | Inline Harness Connector End Views
C316 (4 cavities) | Body wiring harness to the passenger seat heater module wiring harness, under the passenger seat | Harness Routing Views | Inline Harness Connector End Views
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views | --
G301 | Secured to the inside of the lower left B-pillar | Harness Routing Views | --
S230 | IP harness, right side of the IP approximately 4 cm (2 in) from the rear window wiper/washer and multi-function switch breakout | -- | --
S302 | Body harness, right front door approximately 7 cm (3 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S333 | Body harness, front of the left B-pillar approximately 39 cm (15 in) from the G301 breakout | -- | --
S350 | In the Pigtail for the Heater--Seat Cusion--Driver, approximately 12.7 cm (5 in) from the connector for the Seat Heater Module--Driver. | -- | --
S351 | In the Pigtail for the Heater--Seat Cusion--Driver, approximately 2.5 cm (1 in) from the connector for the Seat Heater Module--Driver. | -- | --
S352 | In the Pigtail for the Heater--Seat Cusion--Driver, approximately 12.7 cm (5 in) from the connector for the Seat Heater Module--Driver. | -- | --
S353 | In the Pigtail for the Heater--Seat Cusion--Driver, approximately 2.5 cm (1 in) from the connector for the Seat Heater Module--Driver. | -- | --