For 1990-2009 cars

Problem | Action
--- | ---
The ride is too soft. | Inspect for the following conditions:

• | Wear or damage to the strut and the shock absorbers

• | Broken, sagging, or mispositioned springs

The ride is too hard. | Inspect for the following conditions:

• | Strut or shock absorber installation with the incorrect part number

• | Incorrect tire pressure

The vehicle leads/pulls. | Inspect for the following conditions:

• | Mismatched or uneven tires

• | Broken, sagging, or mispositioned springs

• | Radial tire lateral force

• | Incorrect wheel alignment

• | Dragging front brakes

The vehicle body leans or sways in corners. | Inspect for the following conditions:

• | Wear or damage to the strut, the shock absorbers, and the mounting

• | Broken, sagging, or mispositioned springs

• | Signs of vehicle abuse and overloading

• | Incorrect tire pressure

The suspension bottoms. | Inspect for the following conditions:

• | Signs of vehicle abuse and overloading

• | Wear or damage to the strut or the shock absorbers

• | Broken, sagging, or mispositioned springs

Abnormal or excessive tire wear exists. | Inspect for the following conditions:

• | Misaligned wheels

• | Excessive toe or camber

• | Broken, sagging, or mispositioned springs

• | Incorrect tire balance

• | Wear or damage to the strut or to the shock absorbers

• | Signs of vehicle abuse

• | Uneven or excessive loading of the vehicle

• | Incorrect tire pressure

Dog Tracking exists. | Inspect for the following conditions:

• | Wear or damage to the rear suspension and the bushings

• | Damage to the frame and the underbody alignment