For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Wiper/Washer System Check? | -- | Go to Step 2 | Go to Wiper/Washer System Check
2 |

1. Turn the ignition switch to RUN.
2. Turn the wiper switch to OFF.
3. Disconnect the wiper/washer switch connector C201.

Do the wipers park?

--

Go to Step 3

Go to Step 4

3 | Replace the wiper/washer switch. Refer to Multifunction, Turn Signal, and Hazard Switch Replacement - On Vehicle . Did you complete the replacement? | -- | Go to Step 9 | --
4 | Measure the voltage from connector C201 (vehicle side), terminal E2, to ground with a DMM. Does the voltage measure greater than the specified value? | 1.0 V | Go to Step 6 | Go to Step 5
5 | Replace the wiper motor cover. Refer to Wiper Motor Cover Replacement . Did you complete the replacement? | -- | Go to Step 9 | --
6 |

1. Reconnect the wiper/washer switch connector C201.
2. Disconnect the wiper motor connector.
3. Measure the voltage from the wiper motor connector, terminal D, to ground with a digital voltmeter.

Does the voltage measure greater than the specified value?

1.0 V

Go to Step 8

Go to Step 7

7 | Replace the wiper motor cover. Refer to Wiper Motor Cover Replacement . Did you complete the replacement? | -- | Go to Step 9 | --
8 | Repair the short to voltage in CKT 113. Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | -- | Go to Step 9 | --
9 | Operate the system in order to verify the repair. Did you correct the condition? | -- | System OK | Go to Wiper/Washer System Check