For 1990-2009 cars

### Removal Procedure

1. Carefully pull the sliding door garnish molding away from the sliding door in order to release the clips.

Be sure not to damage the garnish molding.

2. Remove the sliding door molding from the sliding door.

### Installation Procedure

1. Align the sliding door garnish molding clips to the holes in the sliding door.
2. Install the sliding door garnish molding to the sliding door.
3. Firmly press the sliding door garnish molding in order to secure the clips to the holes in the door.