For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Door Jamb Switch Screw | 6 N·m | 53 lb in
Electrical Center Mounting Bolt/Screw | 2 N·m | 18 lb in
Fender Upper Edge Screws | 11 N·m | 97 lb in
Front Fender Liner Rear Bottom Bolts | 2 N·m | 18 lb in
Front Fender Liner to Front Bumper Fascia Bolts | 2 N·m | 18 lb in
Fender Splash Shield Screws | 2 N·m | 18 lb in
Fender to Front Bumper Fascia Bolts | 11 N·m | 97 lb in
Fender to Rear Edge Bolts | 11 N·m | 97 lb in
Front End Sheet Metal Diagonal Brace at Upper Tie Bar Bolts | 25 N·m | 18 lb ft
Front End Sheet Metal Diagonal Brace at Wheelhouse Bolt | 47 N·m | 34 lb ft
Grille Screws | 4 N·m | 35 lb in
Hood Hinge to Hood Bolts | 25 N·m | 18 lb ft
Hood Hinge to Upper Fender Rail Bolts | 25 N·m | 18 lb ft
Hood Latch (Primary) at Support Bolts | 25 N·m | 18 lb ft
Hood Latch (Primary) Bolts | 25 N·m | 18 lb ft
Hood Prop Rod Base Bolts | 10 N·m | 89 lb in
Hood Scoop Screws | 6 N·m | 53 lb in
Latch (Secondary) to Hood Bolts | 25 N·m | 18 lb ft