For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Control Arm Nut * | 220 N·m | 162 lb ft
Rear Axle Tie Rod Bolt | 125 N·m | 92 lb ft
Shock Absorber Nut | 85 N·m | 63 lb ft
Wheel Bearing/Hub Bolts (NEW ONLY) | 80 N·m | 59 lb ft
* This is a prevailing torque type fastener. This fastener may be reused ONLY if:

• | The fastener and its counterpart are clean and free from rust

• | The fastener develops a specified amount of torque (drag) against its counterpart prior to the fastener seating.

| Refer to the appropriate service procedure for the prevailing torque value.

If the fastener does not meet these criteria, REPLACE the fastener.