For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

### Removal Procedure

1. Open the front door.
2. Use the J 38778 to remove the front door bottom auxiliary weatherstrip from the front door.

### Installation Procedure

1. Install the push-in retainers to the front door bottom auxiliary weatherstrip.
2. Stretch the front door bottom auxiliary weatherstrip in order to align the push-in retainers to the holes in the front door.
3. Push in firmly to install the front door bottom auxiliary weatherstrip to the front door.
4. Close the front door.