For 1990-2009 cars

### Removal Procedure

1. Turn OFF the ignition.
2. Loosen both clamps on the MAF sensor (1).
3. Remove the air inlet duct from the MAF sensor.
4. Remove the MAF sensor from air filter housing.

### Installation Procedure

1. Carefully install MAF sensor (1) to air inlet grommet.
2. Attach the MAF sensor (1) to air inlet duct and install the air inlet duct.
3. Tighten the MAF sensor clamps.
4. Connect the MAF sensor electrical connector.