For 1990-2009 cars

Condition | Cause | Action
--- | --- | ---
The power sliding door does not operate electrically. |

1. One of the following conditions is causing battery voltage interruption:

• | The vehicle battery was disconnected and reconnected.

• | The vehicle battery was discharged and recharged.

• | The RADIO fuse (located in the underhood accessory wiring junction block) was removed and then replaced.

2. The PSD Diagnostic Mode was entered and is currently active.
3. The B/U LAMP fuse may be open. With this fuse open the module never sees a park input causing the door to be inoperative.

Re-initialize the PSD system. Refer to Power Sliding Door (PSD) Re-Initialization .

The open/close button on one of the following components does not activate the PSD:

• | The overhead console

• | The B-pillar

• | The keyless entry transmitter

There is a malfunction in circuit 1894.

Refer to Power Sliding Door (PSD) Diagnostic System Check .