For 1990-2009 cars

## Front Bumper Fascia Support Replacement Chevrolet

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Use the J 38778 in order to remove the push-in retainers from the front bumper fascia lower support.
3. Remove the front bumper fascia lower support from the front impact bar.

### Installation Procedure

1. Install the front bumper fascia lower support to the front impact bar.
2. Install the push-in retainers to the front bumper fascia lower support.
3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .

## Front Bumper Fascia Support Replacement Oldsmobile

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Use the J 38778 tool in order to remove the push-in retainers from the front bumper fascia lower support.
3. Remove the front bumper fascia lower support from the front impact bar.

### Installation Procedure

1. Install the front bumper fascia lower support to the front impact bar.
2. Install the push-in retainers to the front bumper fascia lower support.
3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .

## Front Bumper Fascia Support Replacement Pontiac

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Use the J 38778 in order to remove the push-in retainers from the front bumper fascia lower support.
3. Remove the front bumper fascia lower support from the front impact bar.

### Installation Procedure

1. Install the front bumper fascia lower support to the front impact bar.
2. Install the push-in retainers to the front bumper fascia lower support.
3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .