For 1990-2009 cars

Both of the driver and the front passenger bucket seats are designed with a dual-side recliner control mechanism. The recliner mechanism is the sole control of the seat back angle. The recliner mechanism is mounted on the inboard side of the seat. Rotate the recliner control knob either clockwise or counterclockwise (to your desired position) in order to control the position of the seat back.

A 6-way power driver's seat is optional. A 4-way manual seat adjuster is standard only on the driver's seat, with a 2-way adjuster standard on the front passenger's seat. A control lever at the front of the seat cushion controls the manual adjustment forward and backward on the 2 and 4-way seats. The 4-way driver's seat also has a vertical position adjustment lever at the right front seat cushion.