For 1990-2009 cars

### Removal Procedure

1. Remove the IP-trim pad. Refer to Instrument Panel Trim Pad Replacement in Instrument Panel Gauges and Console.
2. Remove the right side windshield pillar garnish molding.
3. Unscrew the coaxial cable from the cellular antenna on the windshield.
4. Unscrew the coaxial cable from the VIU/VCU module.
5. Remove the bolt from the ground tab on the right side on the IP.
6. Remove the cable clips which retain the cable to the IP.
7. Remove the coaxial cable from the vehicle.

### Installation Procedure

1. Install the coaxial cable to the vehicle.
2. Instale the cable clips to the IP frame.
3. Install the bolt to the ground tab on the right side on the IP.
4. Install and tighten the coaxial cable to the VIU/VCU module.
5. Retape the cable to the A-pillar.
6. Install and tighten the coaxial cable to the cellular antenna on the windshield.
7. Install the right side windshield pillar garnish molding.
8. Install the IP-trim pad. Refer to Instrument Panel Trim Pad Replacement in Instrument Panel Gauges and Console.