For 1990-2009 cars

### Removal Procedure

1. Remove the automatic transaxle. Refer to Transmission Replacement in Automatic Transaxle - 4T65-E.
2. Remove the engine flywheel bolts and flywheel.
3. Clean the engine flywheel bolt threads and bolt holes.
4. Clean and inspect the engine flywheel. Refer to Engine Flywheel Cleaning and Inspection .

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the engine flywheel and bolts

Tighten
Tighten bolts to 71 N·m (52 lb ft).

2. Install the automatic transaxle. Refer to Transmission Replacement in Automatic Transaxle - 4T65-E.