For 1990-2009 cars

### Testing Procedure

#### Tools Required

J 35667-A Cylinder Leakdown Tester

With the use of air pressure, a cylinder leakage test will aid in the diagnosis. The cylinder leakage test may be used in conjunction with the engine compression test, to isolate the cause of leaking cylinders.

1. Remove the battery ground (negative) cable. Refer to

   Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

   in General Information.
2. Remove the spark plugs. Refer to Ignition System.
3. Install the J 35667-A .
4. Measure each cylinder on the compression stroke, with both valves closed.

Important: It may be necessary to hold the crankshaft balancer bolt, to prevent piston movement.

5. Apply air pressure, using the J 35667-A . Refer to the manufacturer's instructions.
6. Record the cylinder leakage readings for each cylinder.

Important:

• | Normal cylinder leakage is from 12 to 18 percent.

• | Make a note of any cylinder with more leakage than the other cylinders.

• | Any cylinder with 30 percent leakage or more requires service.

7. Inspect the four primary areas, to properly diagnose a leaking cylinder.
8. If air is heard from the intake or exhaust system, perform the following procedure:

• | Remove the valve rocker arm cover of the suspect cylinder head.

- | Ensure that both valves are closed.

- | Inspect the cylinder head for a broken valve spring.

• | Remove the suspect cylinder head and inspect. Refer to Cylinder Head Clean and Inspect .

9. If air is heard from the crankcase system at the crankcase (oil filler tube), perform the following procedure:

• | Remove the piston from the suspect cylinder.

• | Inspect the piston and connecting rod assembly. Refer to Piston, Connecting Rod, and Bearings Clean and Inspect .

• | Inspect the engine block. Refer to Engine Block Clean and Inspect .

10. If bubbles are found in the radiator, perform the following procedure:

• | Remove both cylinder heads and inspect. Refer to Cylinder Head Clean and Inspect .

• | Inspect the engine block. Refer to Engine Block Clean and Inspect .

11. Remove the J 35667-A .
12. Install the spark plugs. Refer to Ignition System.
13. Install the battery ground (negative) cable. Refer to Battery.