For 1990-2009 cars

### Removal Procedure

1. Remove the front door lock module. Refer to Front Door Module Replacement .
2. Disconnect the front door lock actuator electrical connectors.
3. Remove the front door outside handle lock rod bracket.
4. Remove the front door lock actuator screws.
5. Remove the front door lock actuator from the front door lock.

### Installation Procedure

1. position the front door lock actuator to the front door lock.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the front door lock actuator screws.

Tighten
Tighten the screws to 2 N·m (18 lb in).

3. Install the front door outside handle lock rod bracket.
4. Connect the front door lock actuator electrical connectors.
5. Install the front door lock module. Refer to Front Door Module Replacement .