For 1990-2009 cars

### Removal Procedure

1. Relieve fuel system pressure. Refer to Fuel Pressure Relief .
2. Disconnect the fuel pressure regulator vacuum line.
3. Remove the fuel pressure regulator retaining screw.
4. Using a shop towel to catch any spilled fuel, lift and twist the fuel pressure regulator in order to remove the fuel pressure regulator from the fuel rail.
5. Remove the retainer and spacer bracket from rail and discard.
6. Remove the fuel pressure regulator from the engine fuel return pipe.
7. Remove the fuel pressure regulator inlet O-ring and discard.

### Installation Procedure

Caution: Connect the fuel return line before tightening the regulator attaching screw in order to prevent the regulator from rotating. Rotation of the regulator could damage the retainer and spacer bracket and lead to a fuel leak at the regulator inlet.

Notice:

• | Do not use compressed air in order to test or clean a fuel pressure regulator as damage to the fuel pressure regulator may result.

• | Clean the fuel pressure regulator filter screen with gasoline if necessary.

• | Do not immerse the fuel pressure regulator in a solvent bath in order to prevent damage to the fuel pressure regulator.

1. Check the filter screen for contamination. If contaminated, replace the fuel pressure regulator.
2. Lubricate new pressure regulator inlet O-ring with clean engine oil and install on regulator inlet.
3. Install the fuel return pipe to regulator.
4. Install the new retainer and spacer bracket into slot on fuel rail.
5. Install the pressure regulator to fuel rail.

Tighten
Tighten engine fuel return pipe nut to 17 N·m (13 lb ft).

6. Connect the fuel pressure regulator vacuum line.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

7. Install the pressure regulator attaching screw.

Tighten
Tighten pressure regulator attaching screw to 8.5 N·m (76 lb in).

8. Tighten the pressure regulator fuel return pipe nut.

Tighten
Tighten fuel return pipe nut to 17 N·m (13 lb ft).

9. Inspect and verify that retainer and spacer bracket is engaged in slots in fuel rail. Grasp and pull on regulator to ensure that it is properly seated.
10. Install the fuel filler cap.
11. Inspect for fuel leaks using the following procedure:

11.1. | Turn ON the ignition, for 2 seconds.

11.2. | Turn OFF the ignition, for 10 seconds.

11.3. | Turn ON the ignition.

11.4. | Inspect for fuel leaks.