For 1990-2009 cars

### Installation Procedure

#### Tools Required

• | J 28467-500 Engine Support Fixture

• | Two of the J 28467-6A Engine Support Fixture Lift Hook Brackets

• | J 28467-7A Engine Support Fixture Lift Hook

• | J 28467-8A Engine Support Fixture Swivel Lift Hook

• | Two of the J 28467-34 Engine Support Fixture Lift Hook Wing Nuts

1. Disconnect the battery ground (negative) cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.
2. Remove the right engine mount strut. Refer to Engine Mount Strut Replacement in Engine Mechanical.
3. Install the J 28467-500 .
4. Install the spreader bar to the right engine mount strut bracket.
5. Install the spreader bar to the right (rear) engine lift hook.
6. Install the J 28467-6A .
7. Install the J 28467-7A to the left (front) engine lift hook.
8. Install the J 28467-34 .
9. Install the J 28467-6A .
10. Install the J 28467-8A to the spreader bar.
11. Install the J 28467-34 .
12. The complete engine support fixture installed.

### Removal Procedure

#### Tools Required

• | J 28467-500 Engine Support Fixture

• | Two of the J 28467-6A Engine Support Fixture Lift Hook Brackets

• | J 28467-7A Engine Support Fixture Lift Hook

• | J 28467-8A Engine Support Fixture Swivel Lift Hook

• | Two of the J 28467-34 Engine Support Fixture Lift Hook Wing Nuts

1. Remove the J 28467-34 .
2. Remove the J 28467-7A .
3. Remove the J 28467-6A .
4. Remove the J 28467-34 .
5. Remove the J 28467-8A .
6. Remove the J 28467-6A .
7. Remove the J 28467-500 .
8. Install the right engine mount strut. Refer to Engine Mount Strut Replacement in Engine Mechanical.
9. Connect the battery ground (negative) cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.