For 1990-2009 cars

### Removal Procedure

1. Remove the map pocket net attachment, if equipped. Refer to Front Seat Map Pocket Net Replacement .
2. Remove the cup holder, if equipped. Refer to Cupholder Replacement .
3. Remove the finish cover screws.
4. Unsnap the front seat adjuster switch from the finish cover, if equipped.
5. Remove the finish covers from the front seat frame.

### Installation Procedure

1. Snap the front seat adjuster switch to the finish cover, if equipped.
2. Install the finish covers to the front seat frame.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the finish cover screws.

Tighten
Tighten the screws to 2 N·m (18 lb in).

4. Install the cup holder, if equipped. Refer to Cupholder Replacement .
5. Install the map pocket net attachment, if equipped. Refer to Front Seat Map Pocket Net Replacement .