For 1990-2009 cars

1. Install the spring guide to the tilt spring. Lubricate the spring guide with lithium grease.
2. Install the tilt spring (1).

2.1. | Install the tilt spring (1) to the post on the steering column support assembly (2).

2.2. | Secure the tilt spring (1) with locking pliers.

3. Install the upper and lower trim covers. Refer to Steering Column Trim Covers - Assemble - Off Vehicle .