For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Fuel Filler Door Interlock Bracket Retaining Bolts | 25 N·m | 18 lb ft
Fuel Filler Door Screws | 10 N·m | 89 lb in
Fuel Filler Pocket Screws | 10 N·m | 89 lb in
Liftgate Handle Retaining Bolts | 10 N·m | 89 lb in
Liftgate Handle Retaining Nuts | 10 N·m | 89 lb in
Liftgate Hinge Stud Nuts | 25 N·m | 18 lb ft
Liftgate Hinge to Liftgate Retaining Bolts | 25 N·m | 18 lb ft
Liftgate Latch Retaining Bolts | 10 N·m | 89 lb in
Liftgate Latch Striker Retaining Bolts | 25 N·m | 18 lb ft
Liftgate Lock Cylinder Retaining Nuts | 10 N·m | 89 lb in
Liftgate Strut Ball Stud | 25 N·m | 18 lb ft
Liftgate Strut Bracket to Liftgate Retaining Bolts | 10 N·m | 89 lb in
Lower Cargo Net Retainer Nut | 10 N·m | 89 lb in
Lower Liftgate Wedge Retaining Screws | 10 N·m | 89 lb in
Power Rear Quarter Window Actuator Bearing Bushing Retaining Screws | 2 N·m | 18 lb in
Power Rear Quarter Window Actuator Retaining Bolts | 10 N·m | 89 lb in
Pullstrap Retaining Screws | 2 N·m | 18 lb in
Rear Quarter Window Hinge Stud Nuts | 10 N·m | 89 lb in
Rear Quarter Window Latch Retaining Screws | 10 N·m | 89 lb in
Upper Cargo Net Retainer Screws | 2 N·m | 18 lb in
Upper Liftgate Wedge Retaining Screws | 10 N·m | 89 lb in