For 1990-2009 cars

### Removal Procedure

1. Remove the luggage carrier. Refer to Luggage Carrier Replacement .

Caution: Wear safety glasses in order to avoid eye damage.

2. Drill through the luggage carrier rivnut head using a 7.5 mm (0.295 in) drill bit.
3. Remove the rivnut from the roof.

### Installation Procedure

1. Use a 10 mm (0.39 in) drill bit to drill the hole in the roof out.
2. Install a replacement rivnut to the hole in roof using a rivnut tool, or equivalent.
3. Install the luggage carrier. Refer to Luggage Carrier Replacement .