For 1990-2009 cars

#### No Park Range

Checks | Cause
--- | ---
DEFINITION: One of the two following conditions occur:

• | The transmission range selector cannot be moved into Park.

• | The vehicle can move forward or backward more than 1 meter (3 ft) after the transmission range selector is moved into Park.

Manual Linkage | Misadjusted
Differential Carrier Assembly | The park pawl assembly (694) is broken or damaged.
Park Pawl Actuator Assembly |

• | The actuator assembly (800) is damaged.

• | The actuator guide (809) is damaged or debris is present.